{"text_format":"1","workbook":"xlsx","n_sheets":3,"sheets":["Sheet1","Sheet2","Sheet1 (2)"],"not_rendered":{"charts":0,"images":4,"macros":0,"external_links":0,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"Sheet1","index":0,"n_rows":13,"n_cols":18,"rows_kept":13,"cut":false,"hidden":true,"merged":[[6,7,6,9],[6,15,6,17],[12,5,12,9],[12,13,12,17]]}
[]
[]
[]
[]
[]
[]
[null,null,null,null,null,"设计建筑（kWh）","设计建筑（kWh/m2  . a）","基准建筑（kWh/m2  . a）",null,null,null,null,null,"设计建筑（kWh）","设计建筑（kWh/m2  . a）","基准建筑（kWh/m2  . a）"]
[null,null,null,null,"分类","电耗",null,null,"电耗","一次能源消耗",null,null,"分类","电耗",null,null,"电耗","一次能源消耗"]
[null,null,null,7314.07,"供暖",401767.47,{"$f":"F9/D9","v":54.9307663175223},null,1119484.5,{"$f":"I9/D9","v":153.059035530149},null,1092.4,"供暖",44742,{"$f":"N9/L9","v":40.9575247162212},null,157474.12,{"$f":"Q9/L9","v":144.15426583669}]
[null,null,null,7314.07,"制冷",126043.55,{"$f":"F10/D9","v":17.2330248411623},null,113280.29,15.487996423332,null,1092.4,"制冷",27212.7,{"$f":"N10/L9","v":24.9109300622483},null,37957.07,34.746493958257]
[null,null,null,7314.07,"照明",96574.88,{"$f":"F11/D9","v":13.2039862894394},null,124191.72,16.979837491301,null,1092.4,"照明",30280.05,{"$f":"N11/L9","v":27.7188300988649},null,40717.11,37.2730776272428]
[null,null,null,null,"总计（一次能源）",{"$f":"SUM(F9:F11)","v":624385.9},85.367777448124,null,null,185.526869444782,null,null,"总计（一次能源）",{"$f":"SUM(N9:N11)","v":102234.75},93.5872848773343,null,null,216.17383742219]
[null,null,null,null,"相对节能率 η=（E0-E）/E0",{"$f":"(J12-G12)/J12","v":0.539862998262192},null,null,null,null,null,null,"相对节能率 η=（E0-E）/E0",{"$f":"(R12-O12)/R12","v":0.567073953104892}]

{"sheet":"Sheet2","index":1,"n_rows":0,"n_cols":0,"rows_kept":0,"cut":false,"hidden":true,"merged":[]}

{"sheet":"Sheet1 (2)","index":2,"n_rows":10,"n_cols":10,"rows_kept":10,"cut":false,"hidden":false,"merged":[]}
[]
[]
[null,null,null,null,null,null,null,"线性传热系数Ψ"]
[null,null,null,null,null,"序号","外墙-楼板（WF）","外墙-挑空楼板(WA)","门窗左右(WS)","门窗上口(WU)"]
[null,null,null,null,null,1,0.07,0.08,0.1,0.05]
[null,null,null,null,null,2,0.09,0.198,0.14,0.04]
[null,null,null,null,null,3,0.13,0.43]
[null,null,null,null,null,4,0.13]
[null,null,null,null,null,5,0.06]
[null,null,null,null,null,6,0.09]